**Fiat Linea Classic 1.3 Multijet (Diesel)**

|  |  |
| --- | --- |
| City / Highway Mileage | **16.2 kmpl / 19.5 kmpl** |
| Fuel Type | **Diesel** |
| Engine Displacement | **1248 cc** |
| BHP | **75bhp@4000rpm** |
| Torque | **197Nm@1750rpm** |

**PERFORMANCE**

|  |  |
| --- | --- |
| Top Speed | **170 Kmph** |
| Acceleration (0-100 kmph) | **11.14 Seconds** |
| Engine Displacement(cc) | **1248** |
| Maximum Power | **75bhp@4000rpm** |
| Maximum Torque | **197Nm@1750rpm** |
| Engine Description | **1.3-litre 75bhp 16V Multijet Diesel Engine** |
| Turning Radius | **5.4 metres** |
| No. of Cylinders | **4** |
| Drive Type | **FWD** |
| Turbo Charger | **Yes** |
| Super Charger | **No** |
| Valves Per Cylinder | **4** |
| Compression Ratio | **-** |
| Fuel Supply System | **CRDi** |
| Gear box | **5 Speed** |
| Steering Gear Type | **Rack & Pinion** |

**CAPACITY**

|  |  |
| --- | --- |
| Seating Capacity | **5** |
| No of Doors | **4** |
| Length | **4560mm** |
| Width | **1730mm** |
| Height | **1487mm** |
| Ground Clearance | **185mm** |
| Wheel Base | **2603mm** |
| Front Tread | **-** |
| Rear Tread | **-** |
| Kerb Weight | **1210kg** |
| Gross Weight | **-** |
| Front Headroom | **-** |
| Front Legroom | **-** |
| Rear Headroom | **-** |
| Rear Legroom | **-** |
| Fuel Tank Capacity (Liters) | **45** |
| Cargo Volume | **500-litres** |
| Tyre Size | **175/70 R14** |
| Tyre Type | **Tubeless,Radial** |
| Wheel Size | **14 Inch** |
| Alloy Wheel Size | **-** |
| No of Floors | **-** |