**Volvo S60 D4 KINETIC (Diesel)**

|  |  |
| --- | --- |
| City / Highway Mileage | **23.03 kmpl / 27.03 kmpl** |
| Fuel Type | **Diesel** |
| Engine Displacement | **1969 cc** |
| BHP | **181bhp@4250rpm** |
| Torque | **400Nm@1750-2500rpm** |

**PERFORMANCE**

|  |  |
| --- | --- |
| Top Speed | **215 Kmph** |
| Acceleration (0-100 kmph) | **9.2 Seconds** |
| Engine Displacement(cc) | **1969** |
| Maximum Power | **181bhp@4250rpm** |
| Maximum Torque | **400Nm@1750-2500rpm** |
| Engine Description | **2.0-litre 181bhp 16V Turbo Diesel Engine** |
| Turning Radius | **5.65 metres** |
| No. of Cylinders | **4** |
| Drive Type | **FWD** |
| Turbo Charger | **Yes** |
| Super Charger | **No** |
| Valves Per Cylinder | **4** |
| Compression Ratio | **-** |
| Fuel Supply System | **CRDI** |
| Gear box | **8 Speed** |
| Steering Gear Type | **Rack & Pinion** |

**CAPACITY**

|  |  |
| --- | --- |
| Seating Capacity | **5** |
| No of Doors | **4** |
| Length | **4635mm** |
| Width | **2097mm** |
| Height | **1484mm** |
| Ground Clearance | **136mm** |
| Wheel Base | **2776mm** |
| Front Tread | **1588mm** |
| Rear Tread | **1585mm** |
| Kerb Weight | **1652kg** |
| Gross Weight | **2060kg** |
| Front Headroom | **999mm** |
| Front Legroom | **1064mm** |
| Rear Headroom | **951mm** |
| Rear Legroom | **852mm** |
| Fuel Tank Capacity (Liters) | **67** |
| Cargo Volume | **380-litres** |
| Tyre Size | **215/50 R17** |
| Tyre Type | **Tubeless,Radial** |
| Wheel Size | **-** |
| Alloy Wheel Size | **17 Inch** |
| No of Floors | **-** |