**Volvo V40 D3 Kinetic (Diesel)**

|  |  |
| --- | --- |
| City / Highway Mileage | **12.5 kmpl / 16.8 kmpl** |
| Fuel Type | **Diesel** |
| Engine Displacement | **1984 cc** |
| BHP | **150bhp@3500rpm** |
| Torque | **350Nm@1500-2750rpm** |

**PERFORMANCE**

|  |  |
| --- | --- |
| Top Speed | **210 Kmph** |
| Acceleration (0-100 kmph) | **9.3 Seconds** |
| Engine Displacement(cc) | **1984** |
| Maximum Power | **150bhp@3500rpm** |
| Maximum Torque | **350Nm@1500-2750rpm** |
| Engine Description | **2.0-litre 150bhp 20V Turbo Diesel Engine** |
| Turning Radius | **5.45 metres** |
| No. of Cylinders | **5** |
| Drive Type | **FWD** |
| Turbo Charger | **Yes** |
| Super Charger | **No** |
| Valves Per Cylinder | **4** |
| Compression Ratio | **-** |
| Fuel Supply System | **Direct Injection** |
| Gear box | **6 Speed** |
| Steering Gear Type | **Rack & Pinion** |

**CAPACITY**

|  |  |
| --- | --- |
| Seating Capacity | **5** |
| No of Doors | **5** |
| Length | **4369mm** |
| Width | **2041mm** |
| Height | **1420mm** |
| Ground Clearance | **133mm** |
| Wheel Base | **2647mm** |
| Front Tread | **1559mm** |
| Rear Tread | **1546mm** |
| Kerb Weight | **1561kg** |
| Gross Weight | **1980kg** |
| Front Headroom | **984mm** |
| Front Legroom | **1073mm** |
| Rear Headroom | **932mm** |
| Rear Legroom | **847mm** |
| Fuel Tank Capacity (Liters) | **60** |
| Cargo Volume | **324-litres** |
| Tyre Size | **115/90 R16** |
| Tyre Type | **Tubeless,Radial** |
| Wheel Size | **-** |
| Alloy Wheel Size | **16 Inch** |
| No of Floors | **-** |