**Volvo XC60 D4 KINETIC (Diesel)**

|  |  |
| --- | --- |
| City / Highway Mileage | **11.7 kmpl / 14.7 kmpl** |
| Fuel Type | **Diesel** |
| Engine Displacement | **1984 cc** |
| BHP | **181bhp@4250rpm** |
| Torque | **400Nm@1750-2500rpm** |

**PERFORMANCE**

|  |  |
| --- | --- |
| Top Speed | **195 Kmph** |
| Acceleration (0-100 kmph) | **-** |
| Engine Displacement(cc) | **1984** |
| Maximum Power | **181bhp@4250rpm** |
| Maximum Torque | **400Nm@1750-2500rpm** |
| Engine Description | **2.0-litre 181bhp 20V Turbo Diesel Engine** |
| Turning Radius | **5.8 meters** |
| No. of Cylinders | **5** |
| Drive Type | **FWD** |
| Turbo Charger | **Yes** |
| Super Charger | **No** |
| Valves Per Cylinder | **4** |
| Compression Ratio | **-** |
| Fuel Supply System | **CRDi** |
| Gear box | **8 Speed** |
| Steering Gear Type | **Rack & Pinion** |

**CAPACITY**

|  |  |
| --- | --- |
| Seating Capacity | **5** |
| No of Doors | **5** |
| Length | **4644mm** |
| Width | **2120mm** |
| Height | **1713mm** |
| Ground Clearance | **230mm** |
| Wheel Base | **2774mm** |
| Front Tread | **1632mm** |
| Rear Tread | **1586mm** |
| Kerb Weight | **-** |
| Gross Weight | **-** |
| Front Headroom | **1025mm** |
| Front Legroom | **1047mm** |
| Rear Headroom | **1003mm** |
| Rear Legroom | **924mm** |
| Fuel Tank Capacity (Liters) | **70** |
| Cargo Volume | **495-liters** |
| Tyre Size | **235/65 R17** |
| Tyre Type | **Tubeless,Radial** |
| Wheel Size | **-** |
| Alloy Wheel Size | **17 Inch** |
| No of Floors | **-** |